**Monoblocco rotativo Imbottigliatrice Riempimento-Tappatura per olio e liquidi tranquilli +**

**Etichettatrice rotativa adesiva**

Disponiamo di monoblocco rotativo comprensivo di etichettatrice adesiva, facenti parte di una linea di imbottigliamento Olio o liquidi tranquilli, sono stati utilizzati molto poco, acquistati nell’anno 2010.

Sotto specifiche tecniche e foto inerenti, per ulteriori informazioni cliccare sulla letterina in basso.

***Specifiche tecniche:***

- **Imbottigliatrice per olio Monoblocco rotativo:**

* Produzione MAX. 1000 bott./ora da 750cc senza prevacuazione;
* riempimento sottovuoto;
* serbatoio di riempimento di tipo semi-anulare in acciaio inox 18/8, lucidato a specchio esternamente;
* con prevacuazione aria dalla bottiglia in fase di riempimento con pompa ad alto vuoto e colmatura della bottiglia con gas inerte del riempimento



- **Etichettatrice rotativa adesiva:**

* Produzione 2.000 bott./ora.
* completa di sensori rilevamento tappo;
* sistema di applicazione capsula;
* stampante nr. lotto e data di scadenza con numeri e lettere;
* n°2 stazioni di etichettaggio etichetta e controetichetta su due pellicole separate per bt. tonda e quadra ed una stazione di etichettaggio per applicare etichetta girocollo in adesivo;
* Formati supportati: bt. Fiorentina da 750 ml, 500 ml e 250 ml.

**Franco partenza:** Calabria

**Prezzo:** su Richiesta

**Filling-Capping Monobloc rotary bottling oil and liquids quiet + Rotary labeling adhesive**

We have rotary monoblock including adhesive labeling as part of a bottling line oil or liquid quiet, have been used very little, purchased in 2010.

Under the technical specifications and photos related, for more information click on the letter below.

***Specifications:***

- **Oil Bottling Monoblock Rotary:**

• Production MAX. 1000 bott. / Hour 750cc without prevacuation;

• vacuum filling;

• tank filling of semi-annular stainless steel 18/8, mirror polished outside;

• with prevacuation air from the bottle during filling with a high vacuum pump and topping up of the bottle with an inert gas filling



- **Rotary labeling machine sticker:**

• Production 2,000 bottles. / Hr.

• Complete sensor detection cap;

• application system capsule;

• printer nr. lot number and expiration date with numbers and letters;

• 2 labeling stations label and back on two separate films for bt. round and square and a labeling station to apply adhesive label crewneck;

• Supported formats: bt. Fiorentina, 750 ml, 500 ml and 250 ml.

**EX**: Calabria

**Price**: on inquiry